/*************************************************************************
 *
 *  This file is part of ACT dataflow neuro library.
 * It's the testing facility for cell_lib_std.act
 *
 *  Copyright (c) 2022 University of Groningen - Ole Richter  
 *  Copyright (c) 2022 University of Groningen - Hugh Greatorex
 *  Copyright (c) 2022 University of Groningen - Michele Mastella
 *  Copyright (c) 2022 University of Groningen - Madison Cotteret
 *
 *  This source describes Open Hardware and is licensed under the CERN-OHL-W v2 or later
 *
 *  You may redistribute and modify this documentation and make products
 *  using it under the terms of the CERN-OHL-W v2 (https:/cern.ch/cern-ohl).
 *  This documentation is distributed WITHOUT ANY EXPRESS OR IMPLIED
 *  WARRANTY, INCLUDING OF MERCHANTABILITY, SATISFACTORY QUALITY
 *  AND FITNESS FOR A PARTICULAR PURPOSE. Please see the CERN-OHL-W v2
 *  for applicable conditions.
 *
 *  Source location: https://git.web.rug.nl/bics/actlib_dataflow_neuro
 *
 *  As per CERN-OHL-W v2 section 4.1, should You produce hardware based on
 *  these sources, You must maintain the Source Location visible in its
 *  documentation.
 *
 **************************************************************************
 */

import "../../dataflow_neuro/coders.act";
import "../../dataflow_neuro/primitives.act";
import "../../dataflow_neuro/cell_lib_async.act";
import "../../dataflow_neuro/cell_lib_std.act";


import globals;
import std::data;

open std::data;

open tmpl::dataflow_neuro;

defproc decoder_2d_hs_2x4 (avMx1of2<3> in; a1of1 out[8]){
    bool _reset_B; 
    prs {
        Reset => _reset_B-
    }
    power supply;
    supply.vdd = Vdd;
    supply.vss = GND;

    decoder_2d_hs<1,2,2,4,3> decoder(.in = in, .out = out,
        .reset_B = _reset_B, .supply = supply);

    // model the synapse as having automatic pulldown of ack.
    // Needed since still have the timing assumption,
    // that the synapse ack is pulled down pretty soon after its req is removed.
    // Otherwise it starts fighting the line pull down.
    INV_X1 synapses[8];
    PULLDOWN_X4 synapses2[8];
    (i:8:
        synapses[i].a = decoder.out[i].r;
        synapses2[i].a = synapses[i].y; 
        synapses2[i].y = decoder.out[i].a;

        synapses[i].vss = supply.vss;
        synapses[i].vdd = supply.vdd;
        synapses2[i].vss = supply.vss;
        synapses2[i].vdd = supply.vdd;

    )

}


// fifo_decoder_neurons_encoder_fifo e;
decoder_2d_hs_2x4 e; 